# Ethernet (PHY)

## PHY Bitrate

Auto Negotiate: Let the Ethernet interface determine the best speed based on the device facing it.

Force to 100 Mbps: Manually configure the speed of the Ethernet interface to 100 Mbps.

Force to 10 Mbps: Manually configure the speed of the Ethernet interface to 10 Mbps

## PHY Duplex

Auto Negotiate: Let the Ethernet interface determine the best mode based on the device facing it

Full Duplex: Manually configure the mode of the Ethernet interface to Full duplex.

Half Duplex: Manually configure the mode of the Ethernet interface to Half duplex.

Back to Top