Viper Setup Wizard |  |  |  |  |  |

If you keep the default IP address on all units on your network, they will be accessible via
their local Ethernet port. To monitor or change configurations remotely, each unit needs
a unique IP address. This will be the address that you will point your browser to access
these pages in the future.

Changing this address will not affect your application data but the address shall not be
used elsewhere in your network

Enter a unique IP-address for the unit. If you will be administering it from a different IP
subnet, enter the Default Gateway for this network. You do not need to set a Default
Gateway if you will only be connecting to your Vipers from the same IP subnet.

IP Address | (default: 192.168.205.1)
Network Mask | (default: 255.255.255.0)
Default Gateway |

Note:
The symbol indicates that this parameter will require a 'Reset' before it takes effect.