# Neighbor Table Management - Bridge Mode

When the unit is in bridge mode, the user may manage the remote table. Note that the user must "Save" any changes to this page.

## Add Viper Relay Point

The user may add units to the remote table by entering the MAC address and clicking "Add Viper".

## Remote Unit List

This table is updated every time the Viper sends (or receives) data to (or from) that unit.

### Remote Unit MAC

This is the RF MAC address of the remote unit.

### Communication Path

This field indicates the communication path from this unit to the remote. "Direct" means that there is no intervening unit. "Relay Point" means that there is relay point in between.

### Setting

Displays the current setting of this remote and allows the user to change the setting.

Dynamic: This unit was discovered dynamically by the sending or receiving of a packet.

Relay Point: This unit is a static entry in the remote table.

### Delete

Click the "Delete" button next to the remote entry to delete it from the remote list.

Back to Top