# Unit Status

Displays Viper software revision information retrieved from the connected unit. Have this information available if contacting NextGenRF support.

## Station Name

Displays the name of the connected unit. Configured under Home → Basic Settings → Station Name.

## Model Number

Displays the product catalog number.

## LAN IP Address

IP address for this individual unit. Configured under Lan Settings → LAN IP Address

## LAN MAC Address

MAC address for this individual unit.

## Uptime

Displays the amount of time since the unit was last reset. [DD,HH,MM,SS], Days, Hours, Minutes, Seconds

## Unit Status

Displays the status of the Viper and reports any errors.

Have the displayed Unit Status message available if contacting NextGenRF support. This information is also required if returning a unit for service under RMA.

## IP Forwarding Mode

Displays the IP forwarding mode (Bridge or Router). The IP Forwarding Mode can be configured under RF NetWork Settings → RF Network → IP Forwarding Mode.

## Station Mode

Displays if the unit is being used as a Relay point, Access point or Remote. The Station Mode can be configured under RF NetWork Settings → RF Network → Access/Relay point.

## DC Input Voltage

Displays the DC Input Voltage for the unit.

## Transceiver Temperature

Displays the transceiver internal temperature in Celsius or Fahrenheit. Home → Basic Settings

## VPN Status

Global status of the VPN. It can be configured under Security → VPN.

## Refresh

This button will refresh the parameters on the current page.

## Acknowledge Unit Status

This button allows the user to acknowledge and clear errors.

Errors remain stored, even after cycling power, to aid in troubleshooting intermittent faults. Press the "Acknowledge Unit Status" button to return web page displays and Status LED function to normal operation.

Back to Top