## On-line diagnostics Interval

The on-line diagnostic interval is the time interval in which the unit will broadcast the diagnostic string. You can change the version of online diagnostic messages (1: old style, computer readable, 2: new style, human readable). The new style of online diagnostic messages is the same format at the exception all values are human readable. Please refer to the user manual for detailed information about the format of the diagnostic string.

Note 1: Version 3 is used with the external Device Manager tool. Version 3 is not compatible with previous versions so when in use, it must be enabled on all Vipers part of the network.

Note 2: Setting the Interval to 0 seconds will disable the on-line diagnostic reporting.

Note 3: When "Local Copy Only" is enabled, the Viper unit will not piggyback its diagnostic messages over user traffic. The Viper will still output its diagnostic messages over to TCP clients connected to the online diagnostic TCP port.

Back to Top