# Basic Settings

## Station Name

Station name identifier - Enter string up to forty characters in length.

## Power Management

Allow unit to go in a low-power mode when ignition sense switch off

## Auto Reset

Enabled/Disabled (default). Reset the unit at the given frequency.

Unit Reset Interval indicates how long to wait (after power up) before doing a station reset.

## Temperature Setting

Default = Celsius.

Allows the user to select how the temperature will be reported on the Diagnostics web page and in the Online Diagnostic Messages.

## VLAN Mode

When the VLAN module is enabled, each interface can be configured to operate in "tagged" or "untagged" mode.

Untagged: Devices on this interface are not using VLAN tags. Incoming (ingress) packets are tagged with the port VLAN ID (PVID). VLAN tags are removed on outgoing (Egress) packets.

Tagged: Devices on this interface are using VLAN tags. Incoming (ingress) packets are forwarded with their VLAN ID. Outgoing (Egress) packets are also keeping their VLAN tags.

See each interface for more specific VLAN configuration options and details.

## Management VLAN

When management VLAN is enabled, access to the unit will have to be done thought the use of the "Management VLAN ID".

This parameter only applies in bridge mode

## Management VLAN ID

The Management VLAN ID.

Back to Top