Viper Setup Wizard |  |  |  |  |  |

For easy network maintenance, each station receives a unique name.

Station Name |

Bridge mode is recommended for very simple network topologies.
Router mode covers all kinds of network topologies, simple and complex.

IP Forwarding Mode | Bridge Router

Relay Points are used for relaying broadcast information and for forwarding on-line diagnostics
to AP/DG. They must be carefully selected as to reduce traffic in the network

Relay Point | Yes No

Access Point. This is the default gateway (WAN access) of a Viper network. One and only
one access point may be defined for each Viper network! (Routing mode only)

Access Point | Yes No

Multi-Speed Mode. A single communication speed may be selected between units
(Multi-Speed disabled) or varying speeds.

Multi-Speed Mode

Note:
The symbol indicates that this parameter will require a 'Reset' before it takes effect.