Serial | Com Port | Setup Port | VLAN | Advanced |

Com Port
Port | Enable Disable
Speed |
Data bits | 7 8
Stop bits | 1 2
Parity | Odd Even None
DCD Control |
Packet Forwarding Threshold | MARK character time
Flow Control |
Connection Control |
Status:
Advanced Settings | Show Hide

IP Gateway Service Settings
IP Gateway Service | CLI Service Serial/RF bridge - DOX mode Serial/RF bridge - RTS/CTS mode Online Diagnostics Custom
IP Gateway Transport |
Local Port Number # |
Remote IP Address |
Remote Port Number # |
TCP Keepalive | (minutes)
TCP Server Control | One client Replace old client
RTS/CTS mode settings
CTS assertion delay | ms
CTS negation delay | ms
Send all buffered data before negating CTS
Fragment large messages
Discard all buffered data when entering flow control