# RF Status

## RF IP Address

The RF IP address (default: assigned by factory based on the unit's MAC address) is the RF IP address that is used when sending data and control packets in a Viper network. The address can be configured under RF NetWork Settings → RF Network

## RF MAC Address

The RF MAC address (default: assigned by factory).

## Channel Info

The table presents the Transmit Frequency, Receive Frequency, Output Power, Bandwidth, Bit Rate, Modulation programmed in the unit.

## Multi-Speed Mode

When Multi-Speed mode is disabled, the units communicate with each other at a fixed speed. A unit can be set to operate as a Multi-Speed Master or as a Multi-Speed Slave. A unit set to operate in Multi-Speed slave mode matches the speed of the unit set to operate in Multi-Speed master mode. In a network operating with Multi-Speed, there must be at most one Multi-Speed master unit, all other units must operate in Multi-Speed slave mode. The Multi-Speed Mode can be configured under RF NetWork Settings → RF Network.

## Mode

Indicate if the mode of operation (ANSI, ANSI 900, ETSI).

Back to Top