LAN Settings | LAN Settings | DHCP | SNTP | Broadcast Multicast | VLAN | Ethernet(PHY) |

VLAN Configuration
Name | IP Address | PVID (0-4094) 0:Disabled | Mode | Member Of Mgmt VLAN? |
--- | --- | --- | --- | --- | ---
Ethernet |  |  | Tagged Untagged |  |
Virtual 1 |  |  | Tagged Untagged |  |
Virtual 2 |  |  | Tagged Untagged |  |
Virtual 3 |  |  | Tagged Untagged |  |
Virtual 4 |  |  | Tagged Untagged |  |
Virtual 5 |  |  | Tagged Untagged |  |

VLAN Configuration
Mode | Untagged Tagged
Port VLAN ID | PVID (1-4094)
Member Of Management VLAN | Enabled Disabled
Advanced Settings | Show Hide

Tagged Port Advanced Settings

| Silently | Keep | Retag | Tag | Delete
| Drop | Packet | Packet | Packet | Tag
| Packet | Unchanged | With PVID | With PVID |
Ingress Packet
Untagged |  |  |  |  |
VID=0 |  |  |  |  |
VID=PVID |  |  |  |  |
VID!=PVID (VID is in Table) |  |  |  |  |
VID!=PVID (VID is not in Table) |  |  |  |  |
Egress Packet
Untagged |  |  |  |  |
VID=0 |  |  |  |  |
VID=PVID |  |  |  |  |
VID!=PVID (VID is in Table) |  |  |  |  |
VID!=PVID (VID is not in Table) |  |  |  |  |

Untagged Port Advanced Settings

| Silently | Keep | Retag | Tag | Delete
| Drop | Packet | Packet | Packet | Tag
| Packet | Unchanged | With PVID | With PVID |
Ingress Packet
Untagged |  |  |  |  |
VID=0 |  |  |  |  |
VID=PVID |  |  |  |  |
VID!=PVID |  |  |  |  |
Egress Packet
Untagged |  |  |  |  |
VID=0 |  |  |  |  |
VID=PVID |  |  |  |  |
VID!=PVID |  |  |  |  |

VLAN Membership
| (1-4094)
| (1-4094)
VLAN Member Table