Serial | Com Port | Setup Port | VLAN | Advanced |

VLAN Settings
bridge mode only.... |

VLAN Configuration (Setup Port)
Mode | Untagged
Port VLAN ID | PVID (1-4094)
Advanced Settings | Show Hide

Untagged Port Advanced Settings
| Silently | Keep | Retag | Tag | Delete
| Drop | Packet | Packet | Packet | Tag
| Packet | Unchanged | With PVID | With PVID |
Ingress Packet
Untagged |  |  |  |  |
VID=0 |  |  |  |  |
VID=PVID |  |  |  |  |
VID!=PVID |  |  |  |  |
Egress Packet
Untagged |  |  |  |  |
VID=0 |  |  |  |  |
VID=PVID |  |  |  |  |
VID!=PVID |  |  |  |  |

VLAN Configuration (Com Port)
Mode | Untagged
Port VLAN ID | PVID (1-4094)
Advanced Settings | Show Hide

Untagged Port Advanced Settings
| Silently | Keep | Retag | Tag | Delete
| Drop | Packet | Packet | Packet | Tag
| Packet | Unchanged | With PVID | With PVID |
Ingress Packet
Untagged |  |  |  |  |
VID=0 |  |  |  |  |
VID=PVID |  |  |  |  |
VID!=PVID |  |  |  |  |
Egress Packet
Untagged |  |  |  |  |
VID=0 |  |  |  |  |
VID=PVID |  |  |  |  |
VID!=PVID |  |  |  |  |