# Routing Table

## RIPV2

Router Information Protocol v2 - Default = Disabled.

RIPv2 is a dynamic IP routing protocol based on the distance vector algorithm. RIPv2 is only used in Router mode.

## Routing Table

Displays the table of IP routes that are active in the Viper.

### Destination Network

Displays the IP Address and Netmask of a route.

### Gateway

Displays the IP Address and the RF MAC address (if route is pointing to another Viper) of the destination gateway.

### Type

There are three different types of routes:

Connected: Direct physical connection on the Ethernet port.
Static: User-defined routes.
Proprietary: Routes learned by the Viper unit that point to over-the-air ;destinations.

## Routing Entries

This section allows the user to manually enter new routes or delete existing routes.

Back to Top