# SNMP

This section is only available when the appropriate feature key is installed in the Viper. Contact NextGenRF for information about obtaining and installing the SNMP feature.

SNMP (Simple Network Management Protocol) allows the user to access IP statistics and diagnostics from the Viper using third party MIB Browser Software. Traps (or alarms) will be automatically generated whenever the forward or reverse power goes out of specification. These traps can be sent to a user specified IP address or addresses.

## SNMP Agent

Default = Disabled. Enables or disables the internal SNMP agent.

## Read Community

The read community string gives access in read-only to external MIB browsers.

## Read-Write Community

The read-write community string gives access in read-write to external MIB browsers.

## Trap Community

The community string included in SNMP trap packets.

## Trap IP List

This list shows the user programmed IP addresses where the Viper will send SNMP traps. To add an IP Address to the list, select the 'Add' radio button, enter the IP Address into the text box, then click the 'Save' button at the bottom of the page. When the page is refreshed the new IP address will appear in the Trap IP List.
To delete an IP Address from the list, select the 'Delete' radio button, enter the IP Address to delete into the text box, then click the 'Save' button at the bottom of the page.

## MIB

Click on the 'Download mibs.zip' link to download a .zip file that contains links to the SNMP information available in the Viper. The MIB files must be loaded into a third party MIB browser.

Back to Top