RF Network Settings | RF Network | RF Bandwidth Management |  | Global Settings | VLAN | QoS | QoS Statistics |

Contention Settings

Data Retries |  |  | --- |  | --- |  | --- |  | --- |  | --- |  | --- |  |  |
| OFF |  | 1 |  | 2 |  | 3 |  | 5 |  | 10 |  | Custom
Collision Avoidance |  |  | --- |  | --- |  | --- |  | --- |  | --- |  | --- |  |  |
| OFF |  | 512 |  | 256 |  | 128 |  | 64 |  | 0 |  | Custom
Random Backoff |  |  | --- |  | --- |  | --- |  | --- |  | --- |  | --- |  |  |
| OFF |  | 2 |  | 4 |  | 6 |  | 8 |  | 10 |  | Custom

Minimum Latency/ Maximum Throughput | <===========> | Minimum Congestion/ Maximum Reliability |

Additional Settings
Duplicate Packet Removal (Needed for Rx PER) | Enabled Disabled
Bridge Forwarding | Everything IP and ARP types only
Tx Packet Pacing
TCP | ms
UDP | ms
Fragment | ms
Other | ms