## Global Settings

The Global Settings page allows the user to make changes to a single Viper unit or to the entire Viper network. This allows the user to make changes to the remote units' neighbor tables.

Note: Valid only in Router mode

### Delete Station

The user enters the RF MAC Address of the station that needs to be deleted from the Neighbor Table of all Vipers in the network.

### Replace Station

The user enters the old RF MAC Address (the unit that will be replaced) and the new RF MAC Address that will replace the old Viper. This will update the Neighbor Table of all the Vipers in the network.

### Change ND Mode

The user can change the Neighbor Discovery mode of all the Vipers in the network to Manual-Scan, Auto-Scan or Disabled.

### Change TCP Proxy Mode

The user can change the TCP proxy mode of all the Vipers in the network to Enabled or Disabled.

### Clear Neigbor Table

The user can clear the neighbor table of all the Vipers in the network or just the neighbor table of a specific unit.

### Reset Station(s)

This will send a station reset request to a single Viper unit or to the entire Viper network.

### Save Configuration

This will send a save configuration command to a single Viper unit or to the entire Vipers network.

### Get Status

This will send a "get status" command to all Vipers in the network. The status will be displayed on the Network Management -> Status page.

### Single Station

Allows the user to enter a single RF MAC Address of the desired Viper which commands will be sent to. If this option is selected the command will only be sent to one individual Viper instead of being sent to all Vipers in the Network.

### Apply

The commands will not be sent until the "Apply" button is clicked.